{"text_format":"2","workbook":"xlsx","n_sheets":12,"sheets":["Stromversorgung","Bremsmodul","Drehmomentsensor","Drehgeber","Bremsmotor","Signalampel","IPC","MTS-CTRL","MTS-SENS","MTS-BPL","MTS-FLT","MTS-CONNECT"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Stromversorgung","index":0,"n_rows":9,"n_cols":3,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Stecker"]
["Netzanschluss","230V 50Hz","Leitung mit Schukostecker"]
["Netzanschluss","115V 60Hz","Leitung mit Schukostecker"]
["PE","PE","Klemme"]
["Steckdose Prüfling","230/115V AC erdfrei","Schuko"]
["Backplane Anschluss","230/115V AC erdfrei","Klemme"]
["Backplane Anschluss","230V AC, PE","Klemme"]
["Bremsmodul Anschluss Laststromkreis","230V AC, PE","Klemme"]
["Ein-/Ausschaltrelais Prüfling","24V","Klemme"]

{"sheet":"Bremsmodul","index":1,"n_rows":9,"n_cols":4,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker"]
["Bremsmodul Anschluss Laststromkreis","230V AC, PE","X","Klemme "]
["Bremsmodul Anschluss Steuerstromkreis","24V DC","X","Klemme"]
["Motoranschluss","3x 230V","X","RST Stecker"]
["PE","PE","X","Klemme"]
["Frequenzumrichter Digitalansteuerung","8x 24V","X","D-Sub 25"]
["Frequenzumrichter Analogansteuerung","3x 0…10V","X","D-Sub 25"]
["PROG","RS232","proprietär","D-Sub 9"]
["SSI","RS485","SSI","D-Sub 15"]

{"sheet":"Drehmomentsensor","index":2,"n_rows":5,"n_cols":7,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker","Typ","Pin","Name"]
["Drehmomentsensor VCC","24/12V DC","X","581/M16 12-polig","female","F","VCC"]
[{"$nulls":5},"E","GND"]
["Drehmomentsensor Signal RS485_0","RS485","Lorenz","581/M16 12-polig","female","L","RS485 A"]
[{"$nulls":5},"J","RS485 B"]

{"sheet":"Drehgeber","index":3,"n_rows":9,"n_cols":7,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker","Typ","Pin","Name"]
["SSI","RS485","SSI","M23 12-polig","female",1,"GND"]
[{"$nulls":5},2,"DATA+"]
[{"$nulls":5},3,"CLK+"]
[null,"5V",null,null,null,8,"VCC"]
[{"$nulls":5},9,"SET"]
[{"$nulls":5},10,"DATA-"]
[{"$nulls":5},11,"CLK-"]
[{"$nulls":5},12,"V/R"]

{"sheet":"Bremsmotor","index":4,"n_rows":3,"n_cols":3,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Stecker"]
["Motoranschluss","3x 230V","Klemmenkasten"]
["PE","PE","verschraubt"]

{"sheet":"Signalampel","index":5,"n_rows":5,"n_cols":5,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Stecker","Pin","Name"]
["Signalampel Anschluss","4x 24V","Leitung, Litze","grau","LED rot"]
[null,null,null,"gelb","LED gelb"]
[null,null,null,"grün","LED grün"]
[null,null,null,"weiß","GND"]

{"sheet":"IPC","index":6,"n_rows":9,"n_cols":4,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker"]
["USB Tastatur",null,"USB","USB-A"]
["USB Maus",null,"USB","USB-A"]
["Monitor",null,"HDMI/DP","HDMI/DP"]
["Netzteil","24V","X","Rundstecker"]
["RS232_0","RS232","Prüfling","D-Sub 9"]
["RS485_0","RS485","Lorenz","D-Sub"]
["RS485_1","RS485","µC-Interface","D-Sub"]
["RS485_1","RS485","µC-Interface","D-Sub 9"]

{"sheet":"MTS-CTRL","index":7,"n_rows":32,"n_cols":5,"rows_kept":32,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker","Pin"]
["PROG","X","X","B5B"]
["UART2","UART","UART","B4B"]
["SSI","SSI","SSI","B08B"]
["SSI","SSI","SSI","B08B"]
[]
["VCC-DC1","X","X","DIN41612 H7F24","Z16"]
["VCC-DC2","X","X","DIN41612 H7F24","Z14"]
["RS232-RX1","RS232","RS232","DIN41612 H7F24","Z12"]
["RS232-TX1","RS232","RS232","DIN41612 H7F24","Z10"]
["RS232-RX2","RS232","RS232","DIN41612 H7F24","Z8"]
["RS232-TX2","RS232","RS232","DIN41612 H7F24","Z6"]
["RS485-A","RS485","X","DIN41612 H7F24","D14"]
["RS485-B","RS485","X","DIN41612 H7F24","D16"]
["RS485-C","RS485","X","DIN41612 H7F24","D10"]
["RS485-D","RS485","X","DIN41612 H7F24","D12"]
["CAN-H","CAN","CAN ","DIN41612 H7F24","D6"]
["CAN-L","CAN","CAN ","DIN41612 H7F24","D8"]
["HSSW-GND","X","X","DIN41612 H7F24","Z2, D2"]
[]
["GND","X","X","DIN41612 H7F24","B6…B16"]
["PE/GND","X","X","DIN41612 H7F24","Z20, Z32"]
["AC1_L","max. 230V AC","X","DIN41612 H7F24","Z28"]
["AC1_N","max. 230V AC","X","DIN41612 H7F24","Z30"]
["AC2_L","max. 230V AC","X","DIN41612 H7F24","Z24"]
["AC2_N","max. 230V AC","X","DIN41612 H7F24","Z26"]
[]
["AIN",null,null,"D-Sub 25","23,10,22,9"]
["VOUT",null,null,"D-Sub 25","8,20,7"]
["HSSW-OUT",null,null,"D-Sub 25","6,18,5,17,3,15,2,14"]
["VCC24V","24V","X","D-Sub 25",13.25]
["GND","X","X","D-Sub 25","1,16,4,19,21,11,24,12"]

{"sheet":"MTS-SENS","index":8,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker","Pin"]
["PROG","X","X","B5B"]
["UART2","UART","UART","B4B"]
["SPI2","SPI","SPI","TSW-103-07"]
[]
["PE/GND","X","X","DIN41612 H7F24","Z20, Z32"]
["AC-L","230V AC","X","DIN41612 H7F24","Z28"]
["AC-N","230V AC","X","DIN41612 H7F24","D30"]
[]
["RS485-A","RS485","X","DIN41612 H7F24","D14"]
["RS485-B","RS485","X","DIN41612 H7F24","D16"]
[]
["KTYA","X","X","D-Sub 37","1, 20"]
["KTYB","X","X","D-Sub 37","2, 21"]
["PT","X","X","D-Sub 37","3,4,5,6,7,8,9,10,11,12"]
["IN_P","X","X","D-Sub 37","34,35,36,37"]
["IN_N","X","X","D-Sub 37","16,17,18,19"]
["GND","X","X","D-Sub 37","22,23,24,25,26,27,28,29,30,31"]

{"sheet":"MTS-BPL","index":9,"n_rows":40,"n_cols":5,"rows_kept":40,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker","Pin"]
["VCC-DC1","X","X","DIN41612 H7F24","Z16"]
["VCC-DC2","X","X","DIN41612 H7F24","Z14"]
["RS232-RX1","RS232","RS232","DIN41612 H7F24","Z12"]
["RS232-TX1","RS232","RS232","DIN41612 H7F24","Z10"]
["RS232-RX2","RS232","RS232","DIN41612 H7F24","Z8"]
["RS232-TX2","RS232","RS232","DIN41612 H7F24","Z6"]
["RS485-A","RS485","X","DIN41612 H7F24","D14"]
["RS485-B","RS485","X","DIN41612 H7F24","D16"]
["RS485-C","RS485","X","DIN41612 H7F24","D10"]
["RS485-D","RS485","X","DIN41612 H7F24","D12"]
["CAN-H","CAN","CAN ","DIN41612 H7F24","D6"]
["CAN-L","CAN","CAN ","DIN41612 H7F24","D8"]
["not used","X","X","DIN41612 H7F24","Z2"]
["not used","X","X","DIN41612 H7F24","B2"]
["not used","X","X","DIN41612 H7F24","D2"]
["not used","X","X","DIN41612 H7F24","Z4"]
["not used","X","X","DIN41612 H7F24","B4"]
["not used","X","X","DIN41612 H7F24","D4"]
["GND","X","X","DIN41612 H7F24","B6…B16"]
["PE/GND","X","X","DIN41612 H7F24","Z20, Z32"]
["AC1_L","max. 230V AC","X","DIN41612 H7F24","Z28"]
["AC1_N","max. 230V AC","X","DIN41612 H7F24","Z30"]
["AC2_L","max. 230V AC","X","DIN41612 H7F24","Z24"]
["AC2_N","max. 230V AC","X","DIN41612 H7F24","Z26"]
[]
["VCC-DC1","X","X","B4P-VH",1]
["VCC-DC2","X","X","B4P-VH",3]
[]
["RS232-TX2","RS232","RS232","D-Sub 9",6]
["RS232-RX2","RS232","RS232","D-Sub 9",7]
["RS232-TX1","RS232","RS232","D-Sub 9",3]
["RS232-RX1","RS232","RS232","D-Sub 9",2]
["CAN-H","CAN","CAN","D-Sub 9",8]
["CAN-L","CAN","CAN","D-Sub 9",9]
[]
["RS485-B","RS485","X","D-Sub 9",1]
["RS485-A","RS485","X","D-Sub 9",2]
["RS485-D","RS485","X","D-Sub 9",3]
["RS485-C","RS485","X","D-Sub 9",4]

{"sheet":"MTS-FLT","index":10,"n_rows":7,"n_cols":4,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker"]
["U_IN1","U_ZK","X","B2P3"]
["U_IN2","U_ZK","X","B2P3"]
["U_IN3","U_ZK","X","B2P3"]
["U_OUT1","U_ZK","X","B2P3"]
["U_OUT2","U_ZK","X","B2P3"]
["U_OUT3","U_ZK","X","B2P3"]

{"sheet":"MTS-CONNECT","index":11,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[]}
["Schnittstelle","el. Spez.","Protokoll","Stecker","Pin"]
["VCC-DC1","X","X","DIN41612 H7F24","Z16"]
["VCC-DC2","X","X","DIN41612 H7F24","Z14"]
["RS232-RX1","RS232","RS232","DIN41612 H7F24","Z12"]
["RS232-TX1","RS232","RS232","DIN41612 H7F24","Z10"]
["RS232-RX2","RS232","RS232","DIN41612 H7F24","Z8"]
["RS232-TX2","RS232","RS232","DIN41612 H7F24","Z6"]
["RS485-A","RS485","X","DIN41612 H7F24","D14"]
["RS485-B","RS485","X","DIN41612 H7F24","D16"]
["RS485-C","RS485","X","DIN41612 H7F24","D10"]
["RS485-D","RS485","X","DIN41612 H7F24","D12"]
["CAN-H","CAN","CAN ","DIN41612 H7F24","D6"]
["CAN-L","CAN","CAN ","DIN41612 H7F24","D8"]
[]
["GND","X","X","DIN41612 H7F24","B6…B16"]
["PE/GND","X","X","DIN41612 H7F24","Z20, Z32"]
["AC1_L","max. 230V AC","X","DIN41612 H7F24","Z28"]
["AC1_N","max. 230V AC","X","DIN41612 H7F24","Z30"]
["AC2_L","max. 230V AC","X","DIN41612 H7F24","Z24"]
["AC2_N","max. 230V AC","X","DIN41612 H7F24","Z26"]
[]
["RS232.RX1","RS232","RS232","D-Sub 9",2]
["RS232.TX1","RS232","RS232","D-Sub 9",3]
["GND","X","X","D-Sub 9",5]
[]
["RS485A","RS485","X","D-Sub 9",2]
["RS485B","RS485","X","D-Sub 9",1]
["GND","X","X","D-Sub 9",5]
["VCC12V","12V","X","D-Sub 9",4]