{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["BOM_SS21_PRA"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOM_SS21_PRA","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Part Number","Manufacturer","Quantity","Value","Package","Description","Designator","Footprint","Comment"]
["RC0402JR-070RL","Yageo / Phycomp",3,null,null,"","SB1, SB2, SB3","RESC1005X40X25NL05T10","0R"]
["CRCW1206523RFKEA","Vishay Dale",6,null,null,"","R300, R301, R302, R400, R401, R402","RESC3216X60X45NL10T20","4K7, 2K2"]
["BC548B",null,2,null,null,"","Q400, Q401","Transistor-3Pin","BC548B"]
[null,null,1,null,null,"","Knopfzelle","KZH20","KZH20"]
[null,null,1,null,null,"","U200","D1 mini","LOLIN D1 mini"]
[null,null,1,null,null,"Extremely Accurate I2C-Integrated Real-Time Clock/TCXO/Crystal, 16-Pin SO, 0 to 70 degC, RoHS Qualified","U300","W16#H2_N","DS3231S"]
[null,null,1,null,null,"For soldering wires to PCB","","Klemmleiste_5.08mm","BMS_BOARD"]
[null,null,1,null,null,"MOSFET P-CH 20V 2A TO-236AB","Q100","FP-SOT23-MFG","NX2301P,215"]
[null,null,2,null,null,"","J1, J2","Jumper","Jumper"]
[null,null,2,null,null,"","S1, S2","KLEMMLEISTE_2.54MM","Schalter, Pushbutton"]
[null,null,2,"10uF",null,"CAP 10uF 10V ±20% 1206 (3216 Metric) Thickness 1.9mm SMD","C100, C201","CAPC1206(3216)190_L","10uF"]
[null,null,3,"100nF",null,"CAP 100nF 10V ±20% 1206 (3216 Metric) Thickness 1.9mm SMD","C200, C300, C301","CAPC1206(3216)190_L","100nF"]
[null,null,4,null,null,"","MH1, MH2, MH3, MH4","Mounting hole","29mm"]
[null,"OSRAM",1,null,"SFH213","SENSOR PHOTODIODE 850NM RADIAL","D400","FP-SFH213-0","SFH213"]
[null,"Texas Instruments",1,null,null,"CMOS Quad 2-Input NAND Gate, N0014A, TUBE","U100","N0014A","CD4011BE"]